{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["GPIO Pinlist"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"GPIO Pinlist","index":0,"n_rows":15,"n_cols":38,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,11,1,11],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,10,1,10],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,17,0,18],[0,34,0,37],[1,34,1,35],[1,36,1,37],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,31,0,33],[0,19,0,20]]}
["模块管脚位置","模块管脚序号","模块管脚名称","备注","RESET复位电平","可复用GPIO","Item","PIN NO.","GPIO number","Ball Name.","Power Domain","Pull-Up","Pull-Down","Function0",null,"Function1",null,"Function2",null,"Function3",null,"Function4",null,"Function5",null,"Function6",null,"Function7",null,"Function8",null,"Pin Config",null,null,"Pin State"]
[{"$nulls":13},"Function0","Type","Function1","Type","Function2","Type","Function3","Type","Function4","Type","Function5","Type","Function6","Type","Function7","Type","Function8","Type","Drive Strength","At Reset","After Reset","At Reset (H/L/Hiz)",null,"After Reset (H/L/Hiz)"]
["外圈LCC",61,"CAM_PWDN","CAMERA PWDN",null,"gpio19，注意GPIO19只有一个，UART1_RTS和CAM_PWDN都可以配置为GPIO19                            ",null,"K21","GPIO19","CAMPWDN","V_PAD_1V8","20K/4.7K","40K","camera_pwdn","O","i2c_m1_sda","I/O",{"$nulls":4},"gpio_19","I/O",{"$nulls":8},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",57,"CAM_RST","CAMERA RST",null,"gpio18，注意GPIO18只有一个，UART1_CTS和CAM_RTS都可以配置为GPIO18                                ",null,"M19","GPIO18","CAMRSTL","V_PAD_1V8","20K/4.7K","40K","camera_rst_l","O","i2c_m1_scl","O",{"$nulls":4},"gpio_18","I/O",{"$nulls":8},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",56,"CAM_CSI_SLCK","CAMERA_CSI_SLCK",null,"GPIO23，56脚CAMERA_CSI_SLCK与66脚WAKEUP_OUT/I2C3_SDA都可以配置为GPIO23，注意两者互斥，在OPEN CPU中如果使用了56脚CAMERA_CSI_SLCK，WAKEUP_OUT功能将丢失",null,"M22","GPIO23","CAMSCK","V_PAD_1V8","20K/4.7K","40K","spi_camera_sck","O",{"$nulls":4},"spi_lvds_clk","O","gpio_23","I/O",{"$nulls":8},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",55,"CAM_CSI_SI1"," CAMERA_CSI_SI1","低","gpio22，注意GPIO22只有一个，ZSP_UART_TXD/I2C3_SCL和CAM_CSI_SI1都可以配置为GPIO22                                            ",null,"M21","GPIO22","CAMSI1","V_PAD_1V8","20K/4.7K","40K","spi_camera_si_1","I","spi_camera_si_0","I","spi_camera_ssn","O","spi_lvds_cs","O","gpio_22","I/O",{"$nulls":8},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",54,"CAM_CSI_SI0","CAMERA_CSI_SI0","低","gpio21，注意GPIO21只有一个，UART2_TXD和CAM_CSI_SI0都可以配置为GPIO21                                                        ",null,"M20","GPIO21","CAMSIO","V_PAD_1V8","20K/4.7K","40K","spi_camera_si_0","I","spi_camera_si_1","I",null,null,"spi_lvds_do","O","gpio_21","I/O",{"$nulls":8},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",32,"WAKEUP_IN","只用于WAKEUP_IN，不做复用，具体逻辑要求见《休眠与唤醒要求》",null,"GPIO11",null,"Y2","GPIO11","GPO_3","V_PAD_1V8_RTC","20K/4.7K","40K","gpio_11","I/O","spi_1_dio_0","I/O","lte_spi_sclk","O",{"$nulls":6},"gpo_3","O",{"$nulls":4},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",45,"LCD_FMARK","LCD的FMARK",null,"GPIO5",null,"AA18","GPIO5","LCD_FMARK","V_LCD","20K/4.7K/1.8K","50K","lcd_fmark","O","gpio_5",null,"spi_flash1_sio_3","I/O",null,null,"uart_2_txd","O",{"$nulls":8},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",47,"LCD_SDC","LCD的SDC",null,"GPIO1",null,"AA20","GPIO1","SPILCD_SDC","V_LCD","20K/4.7K/1.8K","50K","spi_lcd_sdc","O","gpio_1","I/O","spi_flash1_cs","O","i2c_m3_sda","I/O",{"$nulls":10},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",48,"LCD_CS","LCD的CS",null,"GPIO3",null,"AB20","GPIO3","SPILCD_CS","V_LCD","20K/4.7K/1.8K","50K","spi_lcd_cs","O","gpio_3","I/O","spi_flash1_sio_1","I/O",{"$nulls":12},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",49,"LCD_SIO","LCD的SIO",null,"GPIO0",null,"AB21","GPIO0","SPILCD_SIO","V_LCD","20K/4.7K/1.8K","50K","spi_lcd_sio","I/O","gpio_0","I/O","spi_flash1_clk","O",{"$nulls":12},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",50,"LCD_CLK","LCD的CLK",null,"GPIO2 ",null,"AA21","GPIO2","SPILCD_CLK","V_LCD","20K/4.7K/1.8K","50K","spi_lcd_clk","O","gpio_2","I/O","spi_flash1_sio_0","I/O",{"$nulls":12},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["外圈LCC",51,"LCD_SEL","LCD的SEL",null,"GPIO4   ",null,"AB18","GPIO4","SPILCD_SEL","V_LCD","20K/4.7K/1.8K","50K","spi_lcd_select","O","gpio_4","I/O","spi_flash1_sio_2","I/O",{"$nulls":12},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]
["内圈LGA",151,"SPI1CLK/SD2_CLK","SD2_CLK",null,"GPIO7",null,"AA1","GPIO7","GPIO_7","V_PAD_1V8_RTC","20K/4.7K","40K","gpio_7","I/O","sdmmc2_clk","O","spi_1_clk","O","pwl_out_1","O","wcn_uart_cts","I","wcn_uart_rxd","I",{"$nulls":6},"2/4/6/8","ie=1, oe=0,wpd","ie=1, oe=0,wpd","INPUT","L","INPUT","L"]